{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Лист1"],"not_rendered":{"charts":0,"images":1,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Лист1","index":0,"n_rows":5,"n_cols":9,"rows_kept":5,"cut":false,"hidden":false,"merged":[[1,1,1,4]]}
["Несущая способность деревянной стропильной балки с учетом гниения"]
["Толщина гниения","Основные  размеры балки",null,null,null,"Момент сопротивления с учетом гниения","Расчетное сопротивление древесины изгибу","Несущая способность сечения ","Процент гниения"]
["δгн","b","h","bo","ho"]
[]
[15,20,22,{"$f":"B5-((15*0.1)*2)","v":17},{"$f":"C5-((15*0.1)*2)","v":19},{"$f":"(D5*(E5^2))/6","v":1022.8333333333334},{"$f":"IF(I5>=50,85,130)","v":130},{"$f":"(F5*G5)/100","v":1329.6833333333334},{"$f":"((B5*C5)-(D5*E5))/(D5*E5)*100","v":36.222910216718269}]